使用U盘升级

将固件拷贝到U盘里，U盘插到机器里再开机，开机显示‘UP H’之后会显示升级进度。

升级完成之后断电重启即可。

注意：请勿更改固件名，否则无法识别固件、且不支持NTFS的磁盘格式，建议U盘里只有固件文件。

Copy the firmware file to the USB flash drive, insert the drive into the device and power it on. The display will show UP H upon startup, followed by the upgrade progress bar.

After the upgrade is completed, power off the device and restart it to finish the process.

****Notes****: Do not rename the firmware file, otherwise the device will fail to recognize it. The NTFS file system is ****not supported****. It is recommended that the USB flash drive contains only the firmware file with no other data.